Windows IP Configuration

   Host Name . . . . . . . . . . . . : DESKTOP-Q2O2IPN
   Primary Dns Suffix  . . . . . . . : 
   Node Type . . . . . . . . . . . . : Hybrid
   IP Routing Enabled. . . . . . . . : No
   WINS Proxy Enabled. . . . . . . . : No
   DNS Suffix Search List. . . . . . : hitronhub.home

Ethernet adapter Ethernet:

   Connection-specific DNS Suffix  . : hitronhub.home
   Description . . . . . . . . . . . : Realtek PCIe GbE Family Controller
   Physical Address. . . . . . . . . : 54-AB-3A-46-A9-C3
   DHCP Enabled. . . . . . . . . . . : Yes
   Autoconfiguration Enabled . . . . : Yes
   IPv6 Address. . . . . . . . . . . : fd00:8494:8c8c:8142:d54e:5f4b:4f0a:8d1e(Preferred) 
   Temporary IPv6 Address. . . . . . : fd00:8494:8c8c:8142:916e:2b84:385c:ae57(Preferred) 
   Link-local IPv6 Address . . . . . : fe80::d54e:5f4b:4f0a:8d1e%6(Preferred) 
   IPv4 Address. . . . . . . . . . . : 192.168.0.10(Preferred) 
   Subnet Mask . . . . . . . . . . . : 255.255.255.0
   Lease Obtained. . . . . . . . . . : August 13, 2018 5:45:00 PM
   Lease Expires . . . . . . . . . . : August 20, 2018 5:44:59 PM
   Default Gateway . . . . . . . . . : 192.168.0.1
   DHCP Server . . . . . . . . . . . : 192.168.0.1
   DHCPv6 IAID . . . . . . . . . . . : 72657722
   DHCPv6 Client DUID. . . . . . . . : 00-01-00-01-22-FC-ED-C2-54-AB-3A-46-A9-C3
   DNS Servers . . . . . . . . . . . : 192.168.0.1
   NetBIOS over Tcpip. . . . . . . . : Enabled

Wireless LAN adapter Local Area Connection* 1:

   Media State . . . . . . . . . . . : Media disconnected
   Connection-specific DNS Suffix  . : 
   Description . . . . . . . . . . . : Microsoft Wi-Fi Direct Virtual Adapter
   Physical Address. . . . . . . . . : 16-1C-A8-0D-3A-9B
   DHCP Enabled. . . . . . . . . . . : Yes
   Autoconfiguration Enabled . . . . : Yes

Wireless LAN adapter Local Area Connection* 2:

   Media State . . . . . . . . . . . : Media disconnected
   Connection-specific DNS Suffix  . : 
   Description . . . . . . . . . . . : Microsoft Wi-Fi Direct Virtual Adapter #2
   Physical Address. . . . . . . . . : 26-1C-A8-0D-3A-9B
   DHCP Enabled. . . . . . . . . . . : Yes
   Autoconfiguration Enabled . . . . : Yes

Wireless LAN adapter Wi-Fi:

   Media State . . . . . . . . . . . : Media disconnected
   Connection-specific DNS Suffix  . : hitronhub.home
   Description . . . . . . . . . . . : Qualcomm Atheros AR956x Wireless Network Adapter
   Physical Address. . . . . . . . . : 44-1C-A8-0D-3A-9B
   DHCP Enabled. . . . . . . . . . . : Yes
   Autoconfiguration Enabled . . . . : Yes

Ethernet adapter Bluetooth Network Connection:

   Media State . . . . . . . . . . . : Media disconnected
   Connection-specific DNS Suffix  . : 
   Description . . . . . . . . . . . : Bluetooth Device (Personal Area Network)
   Physical Address. . . . . . . . . : 44-1C-A8-0D-3A-9C
   DHCP Enabled. . . . . . . . . . . : Yes
   Autoconfiguration Enabled . . . . : Yes

Pinging www.google.com [172.217.3.196] with 32 bytes of data:
Reply from 172.217.3.196: bytes=32 time=86ms TTL=56
Reply from 172.217.3.196: bytes=32 time=75ms TTL=56
Reply from 172.217.3.196: bytes=32 time=78ms TTL=56
Reply from 172.217.3.196: bytes=32 time=88ms TTL=56

Ping statistics for 172.217.3.196:
    Packets: Sent = 4, Received = 4, Lost = 0 (0% loss),
Approximate round trip times in milli-seconds:
    Minimum = 75ms, Maximum = 88ms, Average = 81ms

Domain profile configuration:
-------------------------------------------------------------------
Operational mode                  = Enable
Exception mode                    = Enable
Multicast/broadcast response mode = Enable
Notification mode                 = Enable

IMPORTANT: "netsh firewall" is deprecated;
use "netsh advfirewall firewall" instead.
For more information on using "netsh advfirewall firewall" commands
instead of "netsh firewall", see KB article 947709
at https://go.microsoft.com/fwlink/?linkid=121488 .



   MTU  MediaSenseState   Bytes In  Bytes Out  Interface
------  ---------------  ---------  ---------  -------------
4294967295                1          0      15351  Loopback Pseudo-Interface 1
  1500                2    1582832     612130  Wi-Fi
  1500                1  243641099    5522435  Ethernet
  1500                5          0          0  Local Area Connection* 1
  1500                5          0          0  Bluetooth Network Connection
  1500                5          0          0  Local Area Connection* 2

MIB-II IP Statistics
------------------------------------------------------
Forwarding is:                      Disabled
Default TTL:                        128
In Receives:                        95302
In Header Errors:                   0
In Address Errors:                  0
Datagrams Forwarded:                0
In Unknown Protocol:                0
In Discarded:                       3373
In Delivered:                       95604
Out Requests:                       78783
Routing Discards:                   0
Out Discards:                       2
Out No Routes:                      0
Reassembly Timeout:                 60
Reassembly Required:                0
Reassembled Ok:                     0
Reassembly Failures:                0
Fragments Ok:                       0
Fragments Failed:                   0
Fragments Created:                  0